# Bandsaw Induction V1.2

|  |
| --- |
| Operator Name:  Date: |
| |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **Machine identification and setting**  The individual is able to correctly identify, describe and set/adjust the following:   |  |  | | --- | --- | | Saw guides and thrust wheels |  | | Tension device GET TRAINEE TO CHECK BLADE TENSION |  | | Mitre Fence |  | | Type and size of blade |  | | Top and bottom pulley wheel guards |  | | Table angle adjustment |  | | Start and stop controls. |  |   **Machine set up and operation**   |  |  | | --- | --- | | No loose clothing. Hair tied back |  | | Before working, check stop button is functional. |  | | Keep hands 15cm away from blade at all times. |  | | State the maximum size sections that can be safely cut |  | | When cutting radii check bandsaw width is appropriate: <https://www.dakin-flathers.com/blog/how-to-select-bandsaw-blade-width> |  | | Set blade guard ~8mm above workpiece. |  | | Trainee should cut materials to size. |  | | Appropriate use of push sticks. |  | | Use of mitre fence. |  | | Always allow blade to stop before removing workpiece |  | | Only cut round material using a V block. |  | | No lone working. |  | | LEAVE MACHINE IN THE STATE YOU EXPECT TO FIND IT!!!! |  | |  |  | |  |  | |   **Tooling The individual is able to:**   |  |  | | --- | --- | | Identify dull and defective saw blades and teeth |  | | Identify possible blade fracture (clicking) |  | | Knows to report faults to maintenance team. DO NOT CHANGE BLADE |  | |

When competence has been achieved, tick the appropriate requirement.   
For operations not carried out, mark N/A for Not Applicable